**GUARANTEED TECHNICAL PARTICULARS (GTP) TO BE SPECIFIED BY BIDDER:**

|  |  |  |
| --- | --- | --- |
| **Sr. No.** | **Parameters** | **Value to be specified by Bidder** |
| 01 | Trailer Safe working load (MT) |  |
| 02 | Ground clearance (bottom-most part/ flange I-beam) (mm) |  |
| 03 | Axle length (mm) |  |
| 04 | Axle No.s (mm) |  |
| 05 | Tare weight/Self-weight (MT) |  |
|  | **Frame:** |  |
| 06 | Main beams steel (grade) |  |
| 07 | Cross-beam steel (grade) |  |
| 08 | Safety coupling thickness (mm) |  |
| 09 | Top plate steel thickness (mm) & (grade) |  |
|  | **Running gear:** |  |
| 10 | No. of rocker's arms, with a total of No. of oscillating axles and No. of solid rubber tyres |  |
| 11 | Rocker arm (grade), bushing size (mm) |  |
| 13 | Wheel with tyre dimension (inches) |  |
| 14 | No of steel-sealing rings |  |
| 15 | No of heavy-duty conical bearings |  |
| 17 | Drawbar with forged towing eye dia (mm) |  |
| 18 | Drawbar length foldable/ detachable (mm) |  |
| 19 | Tyres:  No of Solid Rubber Tires with dimensions in Ø ….X….. mm |  |
| 20 | Calculated designed breakdown load of the trailer (MT) |  |
| 21 | Maximum deflection under 350MT load (mm) |  |
| 22 | Drawbar height with respect to ground (mm) |  |